**Bridge Deck Construction Checklist During Pour**

|  |  |
| --- | --- |
| PIN: |  |
| County: |  |
| Federal Project No.: |  |
| State Project No.: |  |

Answer “Yes” or “No” except as noted and elaborate on “No” answers. YES NO

1. Are all concrete trucks on the approved list?

2. Is plastic concrete checked several times behind screed for slab

depth and rebar cover and documented?

3. Do pour, finishing operations and deck finish comply with specifications?

4. Do checks of the pour rate indicate it is satisfactory? (at least 20’/hr. along

roadway)

5. Has the deck been straightedged and any deficiencies corrected?

6. Are required tests on concrete made and the data recorded in book and   
on tickets?

7. Is the amount of curing compound checked both before use and after   
deck pour to determine quantity used? Compute rate and show here

in ft.²/gal.

8. Is the curing compound applied as soon as the water sheen disappears

from the surface of the concrete?

9. From a work bridge, is damp burlap placed as soon as surface will   
 support the burlap without undue marring of the concrete?

10. After placement, is the burlap immediately wet with a misty spray and

kept wet thereafter with a continuously fed soaker hose?

11. Is the burlap properly anchored to provide full protection to the concrete?

|  |  |
| --- | --- |
| Inspector: |  |
| Title: |  |
| Date: |  |

Comments: